


**Request packet:**

****


This is a Physical layer for request packet, it contains the number of frame number, frame length, encapsulation type, arrival time.

****


This a data link layer where the destination mac address is c0:f6:ec:90:0b and source mac address is bc:e9:2f:9e:44:14

****

This portion is for Network layer. In this layer the Ip address of source is 172.18.190.9 and destination Ip address is 146.190.62.39


****

This portion is representing the Transport layer. Source port is 60491 and destination port is 80 which is a web port. Header length is 20 byte, checksum is 0X3d60, urgent pointer is 0 this layer is following TCP


****

This is an Application layer. The host is httpforever.com using a persistent connection as the connection: keep-alive header is present.


**Response packet:**

****


This is a Physical layer for request packet, it contains the number of frame number, frame length, encapsulation type, arrival time.

****


This a data link layer where the destination mac address is bc:e9:2f:9e:44:14 and source mac address is c0:f6:ec:90:0b

****

This portion is for Network layer. In this layer the Ip address of source is 146.190.62.39 and destination Ip address is 172.18.190.9

****

This portion is representing the Transport layer. Source port is 80 and destination port is 60491which is a web port. Header length is 20 byte, checksum is 0X5b5a, urgent pointer is 0 this layer is following TCP

****

This is an Application layer. The host is httpforever.com using a persistent connection as the connection: keep-alive header is present. The header status is 304 not modified. The last modification time is also present.